<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="100.33" y1="80.01" x2="0.33" y2="80.01" width="0" layer="20"/>
<wire x1="0.33" y1="80.01" x2="0.33" y2="0.01" width="0" layer="20"/>
<wire x1="0.33" y1="0.01" x2="100.33" y2="0.01" width="0" layer="20"/>
<wire x1="100.33" y1="0.01" x2="100.33" y2="80.01" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="fablab">
<packages>
<package name="R1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="1X01_LONGPAD">
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="02P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="05P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="02P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="FAB_Hello">
<packages>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="001" library="fab" package="SOIC8" value="ATTINY45SI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fablab" package="R1206FAB" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="fablab" package="LED1206FAB" value="YELLOW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="01_SparkFun" package="1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="01_SparkFun" package="1206" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="01_SparkFun" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER_1" library="con-amp-quick" package="02P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="POWER_2" library="con-amp-quick" package="02P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="M05" library="con-amp-quick" package="05P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="01_SparkFun" package="1X01_LONGPAD" value="M01">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fablab" package="R1206FAB" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="fablab" package="LED1206FAB" value="YELLOW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SL1" library="con-amp-quick" package="02P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SL2" library="con-amp-quick" package="03P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="FAB_Hello" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="fablab" package="R1206FAB" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER_3" library="con-amp-quick" package="02P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="001" pad="8"/>
<contactref element="SL2" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="POWER_1" pad="2"/>
<contactref element="POWER_2" pad="2"/>
<contactref element="POWER_3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="001" pad="4"/>
<contactref element="LED" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="POWER_1" pad="1"/>
<contactref element="POWER_2" pad="1"/>
<contactref element="LED1" pad="2"/>
<contactref element="SL2" pad="2"/>
<contactref element="SL1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="POWER_3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="2"/>
<contactref element="LED" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="001" pad="6"/>
<contactref element="M05" pad="4"/>
</signal>
<signal name="RST">
<contactref element="001" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="RST" pad="1"/>
</signal>
<signal name="ADC3">
<contactref element="001" pad="2"/>
<contactref element="M05" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="ADC2">
<contactref element="001" pad="3"/>
<contactref element="M05" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="001" pad="5"/>
<contactref element="M05" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="001" pad="7"/>
<contactref element="R2" pad="1"/>
<contactref element="M05" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="SL1" pad="1"/>
<contactref element="SL2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
